# ibunlock

int ibunlock (int boardDevice);

## Purpose

Releases a lock on a GPIB-ENET board or device. Refer to the iblock function for more information. In general, you should release your lock on a GPIB-ENET connection immediately after you make your critical access.

## Parameters

Input
Name | Type | Description
--- | --- | ---
boardDevice | integer | Device descriptor you obtain from OpenDev, ibfind, or ibdev.

## Return Value

Name | Type | Description
--- | --- | ---
status | integer | Indicates whether the function succeeded.

## See Also

ibunlock