# ATTR_EASY_TAB_BG_COLOR

Data Type: | integer
Description: | The RGB color value used to fill the area behind the tabs. RGB value is a 4-byte integer with the hexadecimal format 0x00RRGGBB, with the respective red, green, and blue components. See MakeColor(). This color defaults to background color of the panel that owns the tab control. If the tabs must be placed over a multi-colored background, then VAL_TRANSPARENT can be specified as the background color at the expense of a small reduction in the speed with which the active tab is changed.
Values: |
VAL_RED | Red = 255, Green = 0, Blue = 0
VAL_GREEN | Red = 0, Green = 255, Blue = 0
VAL_BLUE | Red = 0, Green = 0, Blue = 255
VAL_CYAN | Red = 0, Green = 255, Blue = 255
VAL_MAGENTA | Red = 255, Green = 0, Blue = 255
VAL_YELLOW | Red = 255, Green = 255, Blue = 0
VAL_DK_RED | Red = 128, Green = 0, Blue = 0
VAL_DK_BLUE | Red = 0, Green = 0, Blue = 128
VAL_DK_GREEN | Red = 0, Green = 128, Blue = 0
VAL_DK_CYAN | Red = 0, Green = 128, Blue = 128
VAL_DK_MAGENTA | Red = 255, Green = 0, Blue = 128
VAL_DK_YELLOW | Red = 128, Green = 128, Blue = 0
VAL_LT_GRAY | Red = 192, Green = 192, Blue = 192
VAL_DK_GRAY | Red = 128, Green = 128, Blue = 128
VAL_BLACK | Red = 0, Green = 0, Blue = 0
VAL_WHITE | Red = 255, Green = 255, Blue = 255
VAL_GRAY | Red = 160, Green = 160, Blue = 160
VAL_OFFWHITE | Red = 224, Green = 224, Blue = 224
VAL_TRANSPARENT | Red = 0, Green = 0, Blue = 0, transparent bit set.
VAL_PANEL_GRAY | Red = 192, Green = 192, Blue = 192