Operating Instructions:

1.  Add the cRIO controller that you want to test to the project
2.  Add the File IO folder and the Build Specifications "VIServDist" to the new controller
3.  Deploy the VIServDist to the controller but do not make it a startup app.
4.  Expand the File IO folder and open cRIOBenchmark_Main.vi
5.  Add a folder named "data" to your cRIO local drive
6.  These tests can take hours to run.  Please be patient.

Seeing the results.  Copy the new TDMS result files to your host machine.  The TDMS reader VIs included "ReadTDMS_Report.vi" and "ReadTDMS_FileFormat.vi" let you see streaming performance based on block size.  The first VI graphs performance based on channel configuration and the second VI graphs performance based on file format.  You may need to change your file structure or reader VI to accomodate the new files.

