# DOSColorToRGB

int DOSColorToRGB (int lwDOSColor);

## Purpose

Translates the 16 standard color values from LabWindows for DOS to RGB values as shown in the following table. An RGB value is a 4-byte integer with the hexadecimal format 0x00RRGGBB. RR, GG, and BB are the respective red, green, and blue components of the color value.

LabWindows for DOS | LabWindows/CVI
0 (black) | VAL_BLACK = 0x000000L
1 (dark blue) | VAL_DK_BLUE = 0x000080L
2 (dark green) | VAL_DK_GREEN = 0x008000L
3 (dark cyan) | VAL_DK_CYAN = 0x008080L
4 (dark red) | VAL_DK_RED = 0x800000L
5 (dark magenta) | VAL_DK_MAGENTA = 0x800080L
6 (brown) | VAL_DK_YELLOW = 0x808000L
7 (gray) | VAL_LT_GRAY = 0xC0C0C0L
8 (dark gray) | VAL_DK_GRAY = 0x808080L
9 (blue) | VAL_BLUE = 0x0000FFL
10 (green) | VAL_GREEN = 0x00FF00L
11 (cyan) | VAL_CYAN = 0x00FFFFL
12 (red) | VAL_RED = 0xFF0000L
13 (magenta) | VAL_MAGENTA = 0xFF00FFL
14 (yellow) | VAL_YELLOW = 0xFFFF00L
15 (white) | VAL_WHITE = 0xFFFFFFL

## Parameters

Input
Name | Type | Description
lwDOSColor | integer | One of the 16 standard colors from LabWindows for DOS.

## Return Value

Name | Type | Description
rgbValue | integer | Value indicating the RGB value.