# ATTR_BOTTOM_ACTUAL_RANGE

Type: | Control attribute
Description: | Use this attribute to obtain the effective bottommost range of the splitter control. Several factors determine this value, such as the setting of the ATTR_BOTTOM_RANGE attribute, the size of the panel, the type, size, and position of controls you have attached to the top edge of the splitter, and in what mode they are attached.
Control Types: | Splitters.
Restrictions: | Not settable. Not valid for vertical splitters
Data Type: | integer
Valid Range: | -32768 to 32767