# ATTR_CHECK_RANGE (Control)

Type: | Control attribute
Description: | The type of range checking for the control. When used on a table, it refers to the default state of new cells when ATTR_TABLE_MODE is set to VAL_GRID.
Control Types: | Numerics, numeric slides, tables.
Data Type: | integer
Default Value: | VAL_NOTIFY

Values

VAL_COERCE | The value is coerced to the upper or lower range boundary, whichever is closer.
VAL_IGNORE | The value remains unchanged.
VAL_NOTIFY | Whenever the control is active, the operator is notified with an Out of Range box.