# ATTR_XENG_UNITS

Type: | Control attribute
Description: | The number of engineering units by which to multiply the values shown in the X-axis labels to calculate the actual X values. Example: If the defined range for the graph is -100 to 100 and XENG_UNITS = 2, the X-axis labels range from -1 to 1.
Control Types: | Digital graphs, graphs, strip charts.
Data Type: | integer
Valid Range: | -308 to 308
Default Value: | 0